<html><head><meta name="color-scheme" content="light dark"></head><body><pre style="word-wrap: break-word; white-space: pre-wrap;">% This file gives macros to specify CMYK Color Profiles as supported by Adobe's Acrobat Pro DC software.
% Identifying names, comments and descriptions are taken from AC/DC's "Color Setup" Preferences panel.


% FOGRA39
% "Europe General Purpose 3"
% General-purpose color settings for screen and print in Europe. Profile warnings are disabled.
% Uses the FOGRA39 press characterization. It is designed to produce quality separations for standard ISO printing using: 350% total ink coverage, positive film, and coated paper.
\gdef\FOGRAXXXIX{\setEXTERNALprofile{Coated FOGRA39 \(ISO 12647-2:2004\)}%  /ProfileName
 {Offset commercial and specialty printing according to ISO 12647-2:2004 / Amd 1, paper type 1 or 2 \(gloss or matte coated offset, 115 g/m2\), screen frequency 60/cm.}% /OutputCondition
 {FOGRA39}%  /OutputConditionIdentifier   /OutputCondition (dIDS_OUTPUTCOND_FOGRA39L_long)
 {http://www.color.org}% /RegistryName
 {CMYK}% /ProfileCS
 {02100000}%  /ICCVersion &lt; ... &gt;
 {http://www.adobe.com}% URL
 {Coated FOGRA39 \(ISO 12647-2:2004\)}%  /Info
 {74FF62F330BF0DBE4495B5720542D511}% /CheckSum &lt; ... &gt;
}%  
% sRGB IEC61966-2.1
% Grayscale: Dot Gain 15%
% /OutputIntents[&lt;&lt;/DestOutputProfileRef&lt;&lt;/CheckSum&lt;74FF62F330BF0DBE4495B5720542D511&gt;/ICCVersion&lt;02100000&gt;/ProfileCS(CMYK)/ProfileName(Coated FOGRA39 \(ISO 12647-2:2004\))/URLs[&lt;&lt;/F(http://www.adobe.com)/FS/URL&gt;&gt;]&gt;&gt;/Info(Coated FOGRA39 \(ISO 12647-2:2004\))/OutputCondition(Offset commercial and specialty printing according to ISO 12647-2:2004 / Amd 1, paper type 1 or 2 \(gloss or matte coated offset, 115 g/m2\), screen frequency 60/cm.)/OutputConditionIdentifier(FOGRA39)/RegistryName(http://www.color.org)/S/GTS_PDFX/Type/OutputIntent&gt;&gt;]
% also  "Europe Prepress 3"
% Preparation of content for common printing conditions in Europe. CMYK values are preserved. Profile warnings are enabled.
%  Adobe RGB (1998)
% also  "Europe Web/Internet 2"
% Preparation of content for non-print usage like the World Wide Web (WWW) in Europe. RGB content is converted to sRGB.
% sRGB IEC61966-2.1
% Grayscale: Gray Gamma 2.2


% Coated GRACoL â€” no
% Coated GRACoL 2006 \(ISO 12647-2:2004\)
\gdef\CoatedGRACoL{\setEXTERNALprofile{GRACoL2006_Coated1v2.icc}%  /ProfileName
%{Coated GRACoL 2006 \(ISO 12647-2:2004\)}% 
 {Printing process definition according to ISO 12647-2:2004: Sheetfed Offset Commercial CTP plates ISO 2846-1 Inks - Variable screen frequency / G7 Methodology / grade#1 paper}% /OutputCondition
 {CGATS TR 006}%  /OutputConditionIdentifier   /OutputCondition (dIDS_OUTPUTCOND_CGATSTR006_long)
 {http://www.color.org}% /RegistryName
 {CMYK}% /ProfileCS
 {02000000}%  /ICCVersion &lt; ... &gt;
 {http://www.gracol.org}% URL
 {Coated GRACoL 2006 \(ISO 12647-2:2004\) alpha 1}%  /Info
 {CC7A6196271B13DBAE4622AA1FA0FCA9}% /CheckSum &lt; ... &gt;
}%
%/OutputIntents[&lt;&lt;/DestOutputProfileRef&lt;&lt;/CheckSum&lt;CC7A6196271B13DBAE4622AA1FA0FCA9&gt;/ICCVersion&lt;02000000&gt;/ProfileCS(CMYK)/ProfileName(GRACoL2006_Coated1v2.icc)/URLs[&lt;&lt;/F(http://www.gracol.org)/FS/URL&gt;&gt;]&gt;&gt;/Info(Coated GRACoL 2006 \(ISO 12647-2:2004\) alpha 1)/OutputCondition(Printing process definition according to ISO 12647-2:2004: Sheetfed Offset Commercial CTP plates ISO 2846-1 Inks - Variable screen frequency / G7 Methodology / grade#1 paper)/OutputConditionIdentifier(CGATS TR 006)/RegistryName(http://www.color.org)/S/GTS_PDFX/Type/OutputIntent&gt;&gt;]     does not validate


% ISO Web Coated
% Uses the FOGRA28 press characterization. It is designed to produce quality separations for standard ISO printing using: 350% total ink coverage, positive film, and coated paper.
% Web Coated FOGRA28 \(ISO 12647-2:2004\)
\gdef\ISOWebCoated{\setEXTERNALprofile{ISO Web Coated}%  /ProfileName
%{Web Coated FOGRA28 \(ISO 12647-2:2004\)}%
 {Offset printing according to ISO/DIS 12647-2:2003, OFCOM, paper type 3 = low weight coated web offset, 60 g/m2, screen ruling 60 cm-1, positive-acting plates.}% /OutputCondition
 {FOGRA28}%  /OutputConditionIdentifier    /OutputCondition (dIDS_OUTPUTCOND_FOGRA28L_long)
 {http://www.color.org}% /RegistryName
 {CMYK}% /ProfileCS
 {02400000}%  /ICCVersion &lt; ... &gt;
 {http://www.adobe.com}%{http://www.eci.org}% URL
 %{Web Coated FOGRA28 \(ISO 12647-2:2004\)}%
 {ISO Web Coated}%  /Info
 {0051E65BF3F29BFBB75720217A9C7A5D}% /CheckSum &lt; ... &gt;
}%
%/OutputIntents[&lt;&lt;/DestOutputProfileRef&lt;&lt;/CheckSum&lt;0051E65BF3F29BFBB75720217A9C7A5D&gt;/ICCVersion&lt;02400000&gt;/ProfileCS(CMYK)/ProfileName(ISO Web Coated)/URLs[&lt;&lt;/F(http://www.eci.org)/FS/URL&gt;&gt;]&gt;&gt;/Info(ISO Web Coated)/OutputCondition(Offset printing according to ISO/DIS 12647-2:2003, OFCOM, paper type 3 = low weight coated web offset, 60 g/m2, screen ruling 60 cm-1, positive-acting plates.)/OutputConditionIdentifier(FOGRA28)/RegistryName(http://www.color.org)/S/GTS_PDFX/Type/OutputIntent&gt;&gt;]     does not validate


% Japan Color 2001 Coated
% "Japan General Purpose 2"
% General-purpose color settings for screen and print in Japan. Profile warnings are disabled.
% Uses the Japan Color 2001 specification for type 3 (coated) paper. It is designed to produce quality separations using: 350% total ink coverage, positive film and coated paper.
\gdef\JapanColorMMICoated{\setEXTERNALprofile{Japan Color 2001 Coated}%  /ProfileName
 {Japan Color 2001 Coated: Printing process definition: ISO 12647-2:2004, sheet-fed offset printing, positive plates, paper type 3 \(coated, 105 gsm\), screen frequency 69/cm.}% /OutputCondition
 {JC200103}%  /OutputConditionIdentifier    /OutputCondition(dIDS_OUTPUTCOND_JC200103_long)
 {http://www.color.org}% /RegistryName
 {CMYK}% /ProfileCS
 {02100000}%  /ICCVersion &lt; ... &gt;
 {http://www.adobe.com}% URL
 {Japan Color 2001 Coated}%  /Info
 {4CB167869183B59BBAD20FB90CCF3E0C}% /CheckSum &lt; ... &gt;
}%
% sRGB IEC61966-2.1
% Grayscale: Dot Gain 15%
%/OutputIntents[&lt;&lt;/DestOutputProfileRef&lt;&lt;/CheckSum&lt;4CB167869183B59BBAD20FB90CCF3E0C&gt;/ICCVersion&lt;02100000&gt;/ProfileCS(CMYK)/ProfileName(Japan Color 2001 Coated)/URLs[&lt;&lt;/F(http://www.adobe.com)/FS/URL&gt;&gt;]&gt;&gt;/Info(Japan Color 2001 Coated)/OutputCondition(Japan Color 2001 Coated: Printing process definition: ISO 12647-2:2004, sheet-fed offset printing, positive plates, paper type 3 \(coated, 105 gsm\), screen frequency 69/cm.)/OutputConditionIdentifier(JC200103)/RegistryName(http://www.color.org)/S/GTS_PDFX/Type/OutputIntent&gt;&gt;]
% also "Japan prepress 2"
% Preparation of content for common printing conditions in Japan. CMYK values are preserved. Profile warnings are enabled.
%  Adobe RGB (1998)
% Grayscale: Dot Gain 15%
% also "Japan Web/Internet"
% Preparation of content for non-print usage like the World Wide Web (WWW) in Japan. RGB content is converted to sRGB.
% sRGB IEC61966-2.1
% Grayscale: Gray Gamma 2.2


% Japan Color 2001 Uncoated
% Uses the Japan Color 2001 specification for type 4 (uncoated) paper. It is designed to produce quality separations using: 310% total ink coverage, positive film and uncoated paper.
\gdef\JapanColorMMIUncoated{\setEXTERNALprofile{Japan Color 2001 Uncoated}%  /ProfileName
 {Japan Color 2001 Uncoated: Printing process definition: ISO 12647-2:2004, sheet-fed offset printing, positive plates, paper type 4 \(uncoated, 105 gsm\), screen frequency 69/cm.}% /OutputCondition
 {JCN200104}%  /OutputConditionIdentifier      /OutputCondition(dIDS_OUTPUTCOND_JC200104_long)
 {http://www.color.org}% /RegistryName
 {CMYK}% /ProfileCS
 {02100000}%  /ICCVersion &lt; ... &gt;
 {http://www.adobe.com}% URL
 {Japan Color 2001 Uncoated}%  /Info
 {B4E3FBD4C04CC702A93EB806D974DBF2}% /CheckSum &lt; ... &gt;
}%
%/OutputIntents[&lt;&lt;/DestOutputProfileRef&lt;&lt;/CheckSum&lt;B4E3FBD4C04CC702A93EB806D974DBF2&gt;/ICCVersion&lt;02100000&gt;/ProfileCS(CMYK)/ProfileName(Japan Color 2001 Uncoated)/URLs[&lt;&lt;/F(http://www.adobe.com)/FS/URL&gt;&gt;]&gt;&gt;/Info(Japan Color 2001 Uncoated)/OutputCondition(Japan Color 2001 Uncoated: Printing process definition: ISO 12647-2:2004, sheet-fed offset printing, positive plates, paper type 4 \(uncoated, 105 gsm\), screen frequency 69/cm.)/OutputConditionIdentifier(JC200104)/RegistryName(http://www.color.org)/S/GTS_PDFX/Type/OutputIntent&gt;&gt;]


% Japan Color 2002 Newspaper
% "Japan Color for Newspaper"
% Preparation of content for common newspaper press conditions in Japan. CMYK values are preserved. Profile warnings are enabled.
% Uses the Japan Color 2002 for Newspapers specification. It is designed to produce quality separations using: 240% total ink coverage, positive film and standard newsprint paper.
\gdef\JapanColorMMIINewspaper{\setEXTERNALprofile{Japan Color 2002 Newspaper}%  /ProfileName
 {Japan Color 2002 for Newspaper Printing: Printing process definition: ISO/DIS 12647-3:2004, coldset offset printing, negative plates, newsprint, screen frequency 39/cm.}% /OutputCondition
 {JCN2002}%  /OutputConditionIdentifier     /OutputCondition (dIDS_OUTPUTCOND_JCN2002_long)
 {http://www.color.org}% /RegistryName
 {CMYK}% /ProfileCS
 {02100000}%  /ICCVersion &lt; ... &gt;
 {http://www.adobe.com}% URL
 {Japan Color 2002 Newspaper}%  /Info
 {FA5BE8D5B4EB756BF1399AFC2CDA7D1C}% /CheckSum &lt; ... &gt;
}%
%  Adobe RGB (1998)
% Grayscale: Dot Gain 25%
%OutputIntents[&lt;&lt;/DestOutputProfileRef&lt;&lt;/CheckSum&lt;FA5BE8D5B4EB756BF1399AFC2CDA7D1C&gt;/ICCVersion&lt;02100000&gt;/ProfileCS(CMYK)/ProfileName(Japan Color 2002 Newspaper)/URLs[&lt;&lt;/F(http://www.adobe.com)/FS/URL&gt;&gt;]&gt;&gt;/Info(Japan Color 2002 Newspaper)/OutputCondition(Japan Color 2002 for Newspaper Printing: Printing process definition: ISO/DIS 12647-3:2004, coldset offset printing, negative plates, newsprint, screen frequency 39/cm.)/OutputConditionIdentifier(JCN2002)/RegistryName(http://www.color.org)/S/GTS_PDFX/Type/OutputIntent&gt;&gt;]


% Japan Web Coated (Ad)
% "Japan Magazine Advertisement Color"
% Preparation of content using the Japan Magazine Publisher Association color standard for the Japan magazine and advertising market. CMYK values are preserved. Profile warnings are enabled.
% Uses specifications developed by the Japan Magazine Publisher Association for digital proofing of images in the Japanese magazine/advertising market.
\gdef\JapanWebCoatedAd{\setEXTERNALprofile{Japan Web Coated \(Ad\)}%  /ProfileName
 {Japan Color 2003 for Web Offset: Printing process definition: ISO 12647-2:2004, heat-set web offset printing, positive plates, paper type 3 \(coated, 70 gsm\), screen frequency 69/cm.}% /OutputCondition
 {JCW2003}%  /OutputConditionIdentifier      /OutputCondition (dIDS_OUTPUTCOND_JCW2003_long)
 {http://www.color.org}% /RegistryName
 {CMYK}% /ProfileCS
 {02100000}%  /ICCVersion &lt; ... &gt;
 {http://www.adobe.com}% URL
 {Japan Web Coated \(Ad\)}%  /Info
 {F8607E551233CEFDDA26D7D6BAAA2A4F}% /CheckSum &lt; ... &gt;
}%
%  Adobe RGB (1998)
% Grayscale: Dot Gain 15%
%/OutputIntents[&lt;&lt;/DestOutputProfileRef&lt;&lt;/CheckSum&lt;F8607E551233CEFDDA26D7D6BAAA2A4F&gt;/ICCVersion&lt;02100000&gt;/ProfileCS(CMYK)/ProfileName(Japan Web Coated \(Ad\))/URLs[&lt;&lt;/F(http://www.adobe.com)/FS/URL&gt;&gt;]&gt;&gt;/Info(Japan Web Coated \(Ad\))/OutputCondition(Japan Color 2003 for Web Offset: Printing process definition: ISO 12647-2:2004, heat-set web offset printing, positive plates, paper type 3 \(coated, 70 gsm\), screen frequency 69/cm.)/OutputConditionIdentifier(JCW2003)/RegistryName(http://www.color.org)/S/GTS_PDFX/Type/OutputIntent&gt;&gt;]


% ISO Newspaper (IFRA 26%) â€“ no
\gdef\IFRAXXVI{\setEXTERNALprofile{ISOnewspaper26v4}%  /ProfileName
 {Printing process definition: ISO/DIS 12647-3:2004, Coldset offset printing, contact exposed negative acting plates or computer to plate \(tone value increase of 26\%\), newsprint, screen ruling 40 lines per cm.}% /OutputCondition
 {IFRA26}%  /OutputConditionIdentifier   /OutputCondition (dIDS_OUTPUTCOND_IFRA26_long)
 {http://www.color.org}% /RegistryName
 {CMYK}% /ProfileCS
 {02400000}%  /ICCVersion &lt; ... &gt;
 {http://www.ifra.com}% URL
 {ISOnewspaper26v4}%  /Info
 {BCA21A6AFA3A4B5CEF9CA8E91565C1B7}% /CheckSum &lt; ... &gt;
}%
%/OutputIntents[&lt;&lt;/DestOutputProfileRef&lt;&lt;/CheckSum&lt;BCA21A6AFA3A4B5CEF9CA8E91565C1B7&gt;/ICCVersion&lt;02400000&gt;/ProfileCS(CMYK)/ProfileName(ISOnewspaper26v4)/URLs[&lt;&lt;/F(http://www.ifra.com)/FS/URL&gt;&gt;]&gt;&gt;/Info(ISOnewspaper26v4)/OutputCondition(Printing process definition: ISO/DIS 12647-3:2004, Coldset offset printing, contact exposed negative acting plates or computer to plate \(tone value increase of 26%\), newsprint, screen ruling 40 lines per cm.)/OutputConditionIdentifier(IFRA26)/RegistryName(http://www.color.org)/S/GTS_PDFX/Type/OutputIntent&gt;&gt;]    does not validate


% ISO Newspaper (IFRA 30%) â€“ no
\gdef\IFRAXXX{\setEXTERNALprofile{ISOnewspaper30v4}%  /ProfileName
 {Printing process definition: ISO/DIS 12647-3:2004, Coldset offset printing, contact exposed negative acting plates or computer to plate \(tone value increase of 30\%\), newsprint, screen ruling 40 lines per cm. \(Principally applicable to the USA\).}% /OutputCondition
 {IFRA30}%  /OutputConditionIdentifier    /OutputCondition (dIDS_OUTPUTCOND_IFRA30_long)
 {http://www.color.org}% /RegistryName
 {CMYK}% /ProfileCS
 {02400000}%  /ICCVersion &lt; ... &gt;
 {http://www.ifra.com}% URL
 {ISOnewspaper30v4}%  /Info
 {EE473D92AE08B385A0128F87B0D9EFC0}% /CheckSum &lt; ... &gt;
}%
%/OutputIntents[&lt;&lt;/DestOutputProfileRef&lt;&lt;/CheckSum&lt;EE473D92AE08B385A0128F87B0D9EFC0&gt;/ICCVersion&lt;02400000&gt;/ProfileCS(CMYK)/ProfileName(ISOnewspaper30v4)/URLs[&lt;&lt;/F(http://www.ifra.com)/FS/URL&gt;&gt;]&gt;&gt;/Info(ISOnewspaper30v4)/OutputCondition(Printing process definition: ISO/DIS 12647-3:2004, Coldset offset printing, contact exposed negative acting plates or computer to plate \(tone value increase of 30%\), newsprint, screen ruling 40 lines per cm. \(Principally applicable to the USA\).)/OutputConditionIdentifier(IFRA30)/RegistryName(http://www.color.org)/S/GTS_PDFX/Type/OutputIntent&gt;&gt;]    does not validate


% U.S. Web Coated (SWOP) v2
% "North America General Purpose 2"
% General-purpose color settings for screen and print in North America. Profile warnings are disabled.
\gdef\SWOPCGATSI{\setEXTERNALprofile{U.S. Web Coated \(SWOP\) v2}%  /ProfileName
 {SWOP \(Publication\) printing in USA \(Printing process definition: ANSI CGATS.6\).}% /OutputCondition
 {CGATS TR 001}%  /OutputConditionIdentifier      /OutputCondition(dIDS_OUTPUTCOND_CGATSTR001_long)
 {http://www.color.org}% /RegistryName
 {CMYK}% /ProfileCS
 {02100000}%  /ICCVersion &lt; ... &gt;
 {http://www.adobe.com}% URL
 {U.S. Web Coated \(SWOP\) v2}%  /Info
 {79D7E984EA3AC74EED7CC92BF6B22A0D}% /CheckSum &lt; ... &gt;
}%
% sRGB IEC61966-2.1
% Grayscale: Dot Gain 20%
%/OutputIntents[&lt;&lt;/DestOutputProfileRef&lt;&lt;/CheckSum&lt;79D7E984EA3AC74EED7CC92BF6B22A0D&gt;/ICCVersion&lt;02100000&gt;/ProfileCS(CMYK)/ProfileName(U.S. Web Coated \(SWOP\) v2)/URLs[&lt;&lt;/F(http://www.adobe.com)/FS/URL&gt;&gt;]&gt;&gt;/Info(U.S. Web Coated \(SWOP\) v2)/OutputCondition(SWOP \(Publication\) printing in USA \(Printing process definition: ANSI CGATS.6\).)/OutputConditionIdentifier(CGATS TR 001)/RegistryName(http://www.color.org)/S/GTS_PDFX/Type/OutputIntent&gt;&gt;]
% also  "North America Prepress 2"
% Preparation of content for common printing conditions in North America. CMYK values are preserved. Profile warnings are enabled.
%  Adobe RGB (1998)
% Grayscale: Dot Gain 20%
% also  "North America Web/Internet"
% Preparation of content for non-print usage like the World Wide Web (WWW) in North America. RGB content is converted to sRGB.
% sRGB IEC61966-2.1
% Grayscale: Gray Gamma 2.2
% also "Monitor Color"
% Preparation of content for video and on-screen presentation. Emulates color behavior of most video applications. This setting is not recommended for documents with CMYK data.
% Monitor RGB - Display
% Grayscale: Gray Gamma 2.2


% U.S. Web Coated (SWOP) 3v2 â€“ no
\gdef\SWOPCGATSIII{\setEXTERNALprofile{SWOP2006_Coated3v2.icc}%  /ProfileName
 {Web Offset CTP plates ISO 2846-1 Inks - Variable screen frequency / G7 Methodology / Grade #3 paper}% /OutputCondition
 {CGATS TR 003}%  /OutputConditionIdentifier      /OutputCondition (dIDS_OUTPUTCOND_CGATSTR003_long)
 {http://www.color.org}% /RegistryName
 {CMYK}% /ProfileCS
 {02000000}%  /ICCVersion &lt; ... &gt;
 {http://www.swop.org}% URL
 {Web Coated SWOP 2006 Grade 3 Paper alpha 1}%  /Info
 {7FBAD4C0AE1CB7195C34BFC20E623437}% /CheckSum &lt; ... &gt;
}%
%/OutputIntents[&lt;&lt;/DestOutputProfileRef&lt;&lt;/CheckSum&lt;7FBAD4C0AE1CB7195C34BFC20E623437&gt;/ICCVersion&lt;02000000&gt;/ProfileCS(CMYK)/ProfileName(SWOP2006_Coated3v2.icc)/URLs[&lt;&lt;/F(http://www.swop.org)/FS/URL&gt;&gt;]&gt;&gt;/Info(Web Coated SWOP 2006 Grade 3 Paper alpha 1)/OutputCondition(Web Offset CTP plates ISO 2846-1 Inks - Variable screen frequency / G7 Methodology / Grade #3 paper)/OutputConditionIdentifier(CGATS TR 003)/RegistryName(http://www.color.org)/S/GTS_PDFX/Type/OutputIntent&gt;&gt;]   does not validate


% U.S. Web Coated (SWOP) 5v2 â€“ no
\gdef\SWOPCGATSV{\setEXTERNALprofile{SWOP2006_Coated5v2.icc}%  /ProfileName
 {Web Offset CTP plates ISO 2846-1 Inks - Variable screen frequency / G7 Methodology / grade #5 Paper}% /OutputCondition
 {CGATS TR 005}%  /OutputConditionIdentifier      /OutputCondition (dIDS_OUTPUTCOND_CGATSTR005_long)
 {http://www.color.org}% /RegistryName
 {CMYK}% /ProfileCS
 {02000000}%  /ICCVersion &lt; ... &gt;
 {http://www.swop.org}% URL
 {Web Coated SWOP 2006 Grade 5 Paper alpha 1}%  /Info
 {34F7C3C809B926B173EE54E13D655BEE}% /CheckSum &lt; ... &gt;
}%
%/OutputIntents[&lt;&lt;/DestOutputProfileRef&lt;&lt;/CheckSum&lt;34F7C3C809B926B173EE54E13D655BEE&gt;/ICCVersion&lt;02000000&gt;/ProfileCS(CMYK)/ProfileName(SWOP2006_Coated5v2.icc)/URLs[&lt;&lt;/F(http://www.swop.org)/FS/URL&gt;&gt;]&gt;&gt;/Info(Web Coated SWOP 2006 Grade 5 Paper alpha 1)/OutputCondition(Web Offset CTP plates ISO 2846-1 Inks - Variable screen frequency / G7 Methodology / grade #5 Paper)/OutputConditionIdentifier(CGATS TR 005)/RegistryName(http://www.color.org)/S/GTS_PDFX/Type/OutputIntent&gt;&gt;]    does not validate



% ISO Coated v2 (ECI) â€“ no
\gdef\ISOCoatedECI{\setEXTERNALprofile{ISO Coated v2 \(ECI\)}%  /ProfileName
 {Offset commercial and specialty printing according to ISO 12647-2:2004 / Amd 1, paper type 1 or 2 \(gloss or matte coated offset, 115 g/m2\), screen frequency 60/cm.}% /OutputCondition
 {FOGRA39}%  /OutputConditionIdentifier
 {http://www.color.org}% /RegistryName
 {CMYK}% /ProfileCS
 {02400000}%  /ICCVersion &lt; ... &gt;
 {http://www.eci.org}% URL
 {ISO Coated v2 \(ECI\)}%  /Info
 {BDA07EFCACF5377E91EDACB0454EA7E5}% /CheckSum &lt; ... &gt;
}%
%/OutputIntents[&lt;&lt;/DestOutputProfileRef&lt;&lt;/CheckSum&lt;BDA07EFCACF5377E91EDACB0454EA7E5&gt;/ICCVersion&lt;02400000&gt;/ProfileCS(CMYK)/ProfileName(ISO Coated v2 \(ECI\))/URLs[&lt;&lt;/F(http://www.eci.org)/FS/URL&gt;&gt;]&gt;&gt;/Info(ISO Coated v2 \(ECI\))/OutputCondition(Offset commercial and specialty printing according to ISO 12647-2:2004 / Amd 1, paper type 1 or 2 \(gloss or matte coated offset, 115 g/m2\), screen frequency 60/cm.)/OutputConditionIdentifier(FOGRA39)/RegistryName(http://www.color.org)/S/GTS_PDFX/Type/OutputIntent&gt;&gt;]    does not validate


% US Newsprint (SNAP 2007)
% "North America Newspaper"
% Preparation of content for common newspaper press conditions in Japan. CMYK values are preserved. Profile warnings are enabled.
%  Adobe RGB (1998)
% Grayscale: Dot Gain 25%



% Others available through "Custom"
%  Adobe RGB (1998)
% Grayscale: Dot Gain 15%

% FOGRA27
% Coated FOGRA27 \(ISO 12647-2:2004\)
%Uses the FOGRA27 press characterization. It is designed to produce quality separations for standard ISO printing using: 350% total ink coverage, positive film and coated paper.

% FOGRA28
% Uses the FOGRA28 press characterization. It is designed to produce quality separations for standard ISO printing using: 350% total ink coverage, positive film, and coated paper.
% Web Coated FOGRA28 \(ISO 12647-2:2004\)

% FOGRA29
% Uses the FOGRA29 press characterization. It is designed to produce quality separations for standard ISO printing using: 350% total ink coverage, positive film, and coated paper.
% Uncoated FOGRA29 \(ISO 12647-2:2004\)

% JapanColor2003
% Uses the Japan Color 2003 specification for type 3 (coated) paper. It is designed to produce quality separations using: 350% total ink coverage, positive film and coated paper on heat-set web offset presses.
% Japan Color 2003 Web Coated

% EuroscaleCoated
% Uses specifications designed to produce quality separations using Euroscale inks under the following printing conditions: 350% total area of ink coverage, positive plate, bright white coated stock.
% Euroscale Coated v2

% EuroscaleUnCoated
% Uses specifications designed to produce quality separations using Euroscale inks under the following printing conditions: 260% total area of ink coverage, positive plate, uncoated white offset stock.
% Euroscale Uncoated v2

% US Sheetfed Coated v2

% US Sheetfed UnCoated v2

% US Web UnCoated v2

% Generic CMYK Profile




\endinput



/Library/Application Support/Adobe/Color
/Library/Application Support/Adobe/Color/Profiles
/Library/Application Support/Adobe/Color/Profiles/BlackWhite.icc
/Library/Application Support/Adobe/Color/Profiles/CIERGB.icc
/Library/Application Support/Adobe/Color/Profiles/EuroscaleCoated.icc
/Library/Application Support/Adobe/Color/Profiles/EuroscaleUncoated.icc
/Library/Application Support/Adobe/Color/Profiles/PAL_SECAM.icc
/Library/Application Support/Adobe/Color/Profiles/Recommended
/Library/Application Support/Adobe/Color/Profiles/Recommended/AdobeRGB1998.icc
/Library/Application Support/Adobe/Color/Profiles/Recommended/AppleRGB.icc
/Library/Application Support/Adobe/Color/Profiles/Recommended/CoatedFOGRA27.icc
/Library/Application Support/Adobe/Color/Profiles/Recommended/CoatedFOGRA39.icc
/Library/Application Support/Adobe/Color/Profiles/Recommended/CoatedGRACoL2006.icc
/Library/Application Support/Adobe/Color/Profiles/Recommended/ColorMatchRGB.icc
/Library/Application Support/Adobe/Color/Profiles/Recommended/JapanColor2001Coated.icc
/Library/Application Support/Adobe/Color/Profiles/Recommended/JapanColor2001Uncoated.icc
/Library/Application Support/Adobe/Color/Profiles/Recommended/JapanColor2002Newspaper.icc
/Library/Application Support/Adobe/Color/Profiles/Recommended/JapanColor2003WebCoated.icc
/Library/Application Support/Adobe/Color/Profiles/Recommended/JapanWebCoated.icc
/Library/Application Support/Adobe/Color/Profiles/Recommended/ProPhoto.icm
/Library/Application Support/Adobe/Color/Profiles/Recommended/USNewsprintSNAP2007.icc
/Library/Application Support/Adobe/Color/Profiles/Recommended/USSheetfedCoated.icc
/Library/Application Support/Adobe/Color/Profiles/Recommended/USSheetfedUncoated.icc
/Library/Application Support/Adobe/Color/Profiles/Recommended/USWebCoatedSWOP.icc
/Library/Application Support/Adobe/Color/Profiles/Recommended/USWebUncoated.icc
/Library/Application Support/Adobe/Color/Profiles/Recommended/UncoatedFOGRA29.icc
/Library/Application Support/Adobe/Color/Profiles/Recommended/WebCoatedFOGRA28.icc
/Library/Application Support/Adobe/Color/Profiles/Recommended/WebCoatedSWOP2006Grade3.icc
/Library/Application Support/Adobe/Color/Profiles/Recommended/WebCoatedSWOP2006Grade5.icc
/Library/Application Support/Adobe/Color/Profiles/Recommended/sRGB Color Space Profile.icm
/Library/Application Support/Adobe/Color/Profiles/SMPTE-C.icc
/Library/Application Support/Adobe/Color/Profiles/WideGamutRGB.icc
/Library/Application Support/Adobe/Color/Settings
/Library/Application Support/Adobe/Color/Settings/Europe General Purpose 3.csf
/Library/Application Support/Adobe/Color/Settings/Europe Prepress 3.csf
/Library/Application Support/Adobe/Color/Settings/Europe Web Internet 2.csf
/Library/Application Support/Adobe/Color/Settings/Japan General Purpose.csf
/Library/Application Support/Adobe/Color/Settings/Japan Magazine.csf
/Library/Application Support/Adobe/Color/Settings/Japan Newspaper.csf
/Library/Application Support/Adobe/Color/Settings/Japan Prepress.csf
/Library/Application Support/Adobe/Color/Settings/Japan Web Internet.csf
/Library/Application Support/Adobe/Color/Settings/Monitor Color.csf
/Library/Application Support/Adobe/Color/Settings/North America General Purpose.csf
/Library/Application Support/Adobe/Color/Settings/North America Newspaper.csf
/Library/Application Support/Adobe/Color/Settings/North America Prepress.csf
/Library/Application Support/Adobe/Color/Settings/North America Web Internet.csf



</pre></body></html>